1. **Write an assembly language program for subtracting two 16-bit datausing 8086 processor.**

LDA 0000

MOV B,A

LDA 0001

MOV C,A

LDA 0002

MOV D,A

LDA 0003

SUB C

STA 0005

MOV A,D

SUB B

STA 0004

HLT

